C06B21/00	7	Apparatus or methods for working-up explosives, e.g. forming, cutting, drying<br><br><u>NOTE</u><br><br> In the absence of an indication to the contrary a process is classified in the last appropriate place, e.g. granulation by extrusion and chopping C06B21/0075)]	C06B21/00	C06B21/00		801
C06B21/0008	8	{Compounding the ingredient}	C06B21/00	C06B21/00		962
C06B21/0016	9	{the ingredient being nitrocellulose or oranitro cellulose based propellant; Working up; gelatinising; stabilising (stabilising of explosives in general C06B21/0091)}	C06B21/00	C06B21/00		78
C06B21/0025	9	{the ingredient being a polymer bonded explosive or thermic component}	C06B21/00	C06B21/00		287
C06B21/0033	8	{Shaping the mixture}	C06B21/00	C06B21/00		383
C06B21/0041	9	{by compression}	C06B21/00	C06B21/00		326
C06B21/005	9	{By a process involving melting at least part of the ingredients}	C06B21/00	C06B21/00		262
C06B21/0058	9	{by casting a curable composition, e.g. of the plastisol type}	C06B21/00	C06B21/00		299
C06B21/0066	9	{by granulation, e.g. flaking}	C06B21/00	C06B21/00		637
C06B21/0075	9	{by extrusion}	C06B21/00	C06B21/00		246
C06B21/0083	8	{Treatment of solid structures, e.g. for coating or impregnating with a modifier (compositions therefor C06B23/00)}	C06B21/00	C06B21/00		678
C06B21/0091	8	{Elimination of undesirable or temporary components of an intermediate or finished product, e.g. making porous or low density products, purifying, stabilising, drying; Deactivating; Reclaiming; (porous inert particles or chemicals compounded for these purposes C06B23/00)}	C06B21/00	C06B21/00		704
C06B23/00	7	Compositions characterised by non-explosive or non-thermic constituents {(in combination with specific explosives C06B25/20, C06B25/26, C06B29/04, C06B29/08, C06B31/06, C06B31/40, C06B33/02)}	C06B23/00	C06B23/00		666
C06B23/001	8	{Fillers, gelling and thickening agents (e.g. fibres) , absorbents for nitroglycerine (binders, plasticisers for propellants C06B45/10; crosslinking or curing agents C06B45/10)}	C06B23/00	C06B23/00		580
C06B23/002	8	{Sensitisers or density reducing agents, foam stabilisers, crystal habit modifiers}	C06B23/00	C06B23/00		139
C06B23/003	9	{Porous or hollow inert particles (preparation C06B21/0091)}	C06B23/00	C06B23/00		139
C06B23/004	9	{Chemical sensitisers}	C06B23/00	C06B23/00		103
C06B23/005	8	{Desensitisers, phlegmatisers (coolants for mining explosives C06B23/04; deactivating C06B21/0091)}	C06B23/00	C06B23/00		276
C06B23/006	8	{Stabilisers (e.g. thermal stabilisers) (processes C06B21/0091; foam stabilisers C06B23/002)}	C06B23/00	C06B23/00		307
C06B23/007	8	{Ballistic modifiers, burning rate catalysts, burning rate depressing agents, e.g. for gas generating}	C06B23/00	C06B23/00		785
C06B23/008	8	{Tagging additives}	C06B23/00	C06B23/00		83
C06B23/009	8	{Wetting agents, hydrophobing agents, dehydrating agents, antistatic additives, viscosity improvers, antiagglomerating agents, grinding agents and other additives for working up}	C06B23/00	C06B23/00		426
C06B23/02	8	for neutralising poisonous gases from explosives produced during blasting	C06B23/02	C06B23/02		91
C06B23/04	8	for cooling the explosion gases {including antifouling and flash suppressing agents}	C06B23/04	C06B23/04		359
C06B25/00	7	Compositions containing a nitrated organic compound	C06B25/00	C06B25/00		471
C06B25/02	8	the nitrated compound being starch or sugar	C06B25/02	C06B25/02		117
C06B25/04	8	the nitrated compound being an aromatic	C06B25/04	C06B25/04		398
C06B25/06	9	with two or more nitrated aromatic compounds present	C06B25/06	C06B25/06		60
C06B25/08	10	at least one of which is nitrated toluene	C06B25/08	C06B25/08		35
C06B25/10	8	the compound being nitroglycerine	C06B25/10	C06B25/10		135
C06B25/12	9	with other nitrated organic compounds	C06B25/12	C06B25/12		39
C06B25/14	10	the other compound being a nitrated aliphatic diol	C06B25/14	C06B25/14		7
C06B25/16	10	the other compound being a nitrated aromatic	C06B25/16	C06B25/16		16
C06B25/18	8	the compound being nitrocellulose present as 10% or more by weight of the total composition	C06B25/18	C06B25/18		268
C06B25/20	9	with a non-explosive or a non-explosive or a non-thermic component	C06B25/20	C06B25/20		140
C06B25/22	9	with a nitrated aromatic compound	C06B25/22	C06B25/22		52
C06B25/24	9	with nitroglycerine	C06B25/24	C06B25/24		128
C06B25/26	10	with an organic non-explosive or an organic non-thermic component	C06B25/26	C06B25/26		151
C06B25/28	8	the compound being nitrocellulose present as less than 10% by weight of the total composition	C06B25/28	C06B25/28		26
C06B25/30	9	with nitroglycerine	C06B25/30	C06B25/30		84
C06B25/32	8	the compound being nitrated pentaerythritol	C06B25/32	C06B25/32		165
C06B25/34	8	the compound being a nitrated acyclic, alicyclic or heterocyclic amine	C06B25/34	C06B25/34		1367
C06B25/36	8	the compound being a nitroparaffin	C06B25/36	C06B25/36		152
C06B25/38	9	with other nitrated organic compound	C06B25/38	C06B25/38		32
C06B25/40	9	with two or more nitroparaffins present	C06B25/40	C06B25/40		48
C06B27/00	7	Compositions containing a metal, boron, silicon, selenium or tellurium or mixtures, intercompounds or hydrides thereof, and hydrocarbons or halogenated hydrocarbons	C06B27/00	C06B27/00		532
C06B29/00	7	Compositions containing an inorganic oxygen-halogen salt, e.g. chlorate, perchlorate	C06B29/00	C06B29/00		118
C06B29/02	8	of an alkali metal	C06B29/02	C06B29/02		106
C06B29/04	9	with an inorganic non-explosive or an inorganic non-thermic component	C06B29/04	C06B29/04		67
C06B29/06	10	the component being a cyanide; the component being an oxide of iron, chromium or manganese	C06B29/06	C06B29/06		35
C06B29/08	9	with an organic non-explosive or an organic non-thermic component	C06B29/08	C06B29/08		165
C06B29/10	10	the component being a dye or a colouring agent	C06B29/10	C06B29/10		44
C06B29/12	9	with carbon or sulfur	C06B29/12	C06B29/12		52
C06B29/14	9	with iodine or an iodide	C06B29/14	C06B29/14		10
C06B29/16	9	with a nitrated organic compound	C06B29/16	C06B29/16		56
C06B29/18	10	the compound being nitrated toluene or a nitrated phenol	C06B29/18	C06B29/18		39
C06B29/20	10	the compound being nitrocellulose	C06B29/20	C06B29/20		26
C06B29/22	8	the salt being ammonium perchlorate	C06B29/22	C06B29/22		332
C06B31/00	7	Compositions containing an inorganic nitrogen-oxygen salt	C06B31/00	C06B31/00		238
C06B31/02	8	the salt being an alkali metal or an alkaline earth metal nitrate	C06B31/02	C06B31/02		159
C06B31/04	9	with carbon or sulfur	C06B31/04	C06B31/04		108
C06B31/06	10	with an organic non-explosive or an organic non-thermic component	C06B31/06	C06B31/06		74
C06B31/08	9	with a metal oxygen-halogen salt, e.g. inorganic chlorate, inorganic perchlorate	C06B31/08	C06B31/08		48
C06B31/10	10	with carbon or sulfur	C06B31/10	C06B31/10		64
C06B31/12	9	with a nitrated organic compound	C06B31/12	C06B31/12		55
C06B31/14	10	the compound being an aromatic	C06B31/14	C06B31/14		19
C06B31/16	11	the compound being a nitrated toluene	C06B31/16	C06B31/16		14
C06B31/18	11	the compound being a nitrated phenol, e.g. picric acid	C06B31/18	C06B31/18		8
C06B31/20	10	the compound being nitroglycerine	C06B31/20	C06B31/20		46
C06B31/22	10	the compound being nitrocellulose	C06B31/22	C06B31/22		20
C06B31/24	11	with other explosive or thermic component	C06B31/24	C06B31/24		12
C06B31/26	12	the other component being nitroglycerine	C06B31/26	C06B31/26		7
C06B31/28	8	the salt being ammonium nitrate	C06B31/28	C06B31/28		399
C06B31/285	9	{with fuel oil, e.g. ANFO-compositions}	C06B31/28	C06B31/28		446
C06B31/30	9	with vegetable matter; with resin; with rubber	C06B31/30	C06B31/30		305
C06B31/32	9	with a nitrated organic compound	C06B31/32	C06B31/32		172
C06B31/34	10	the nitrated compound being starch or sugar	C06B31/34	C06B31/34		11
C06B31/36	11	with other explosive or thermic component	C06B31/36	C06B31/36		6
C06B31/38	10	the nitrated compound being an aromatic	C06B31/38	C06B31/38		28
C06B31/40	11	with an organic non-explosive or an organic non-thermic component	C06B31/40	C06B31/40		24
C06B31/42	11	with other explosive or thermic component	C06B31/42	C06B31/42		44
C06B31/44	10	the compound being nitroglycerine	C06B31/44	C06B31/44		18
C06B31/46	11	with a vegetable matter component, e.g. wood pulp, sawdust	C06B31/46	C06B31/46		31
C06B31/48	11	with other explosive or thermic component	C06B31/48	C06B31/48		29
C06B31/50	12	the other component being a nitrated organic compound	C06B31/50	C06B31/50		7
C06B31/52	10	the compound being nitrocellulose present as 10% or more by weight of the total composition	C06B31/52	C06B31/52		24
C06B31/54	11	with other nitrated organic compound	C06B31/54	C06B31/54		13
C06B31/56	10	the compound being nitrocellulose present as less than 10% by weight of the total composition	C06B31/56	C06B31/56		35
C06B33/00	7	Compositions containing particulate metal, alloy, boron, silicon, selenium or tellurium with at least one oxygen supplying material which is either a metal oxide or a salt, organic or inorganic, capable of yielding a metal oxide	C06B33/00	C06B33/00		686
C06B33/02	8	with an organic non-explosive or an organic non-thermic component	C06B33/02	C06B33/02		228
C06B33/04	8	the material being an inorganic nitrogen-oxygen salt	C06B33/04	C06B33/04		233
C06B33/06	8	the material being an inorganic oxygen-halogen salt	C06B33/06	C06B33/06		410
C06B33/08	8	with a nitrated organic compound	C06B33/08	C06B33/08		241
C06B33/10	9	the compound being an aromatic	C06B33/10	C06B33/10		43
C06B33/12	8	the material being two or more oxygen-yielding compounds	C06B33/12	C06B33/12		257
C06B33/14	9	at least one being an inorganic nitrogen-oxygen salt	C06B33/14	C06B33/14		184
C06B35/00	7	Compositions containing a metal azide	C06B35/00	C06B35/00		253
C06B37/00	7	Compositions containing a metal fulminate	C06B37/00	C06B37/00		38
C06B37/02	8	with a nitrated organic compound or an inorganic oxygen-halogen salt	C06B37/02	C06B37/02		24
C06B39/00	7	Compositions containing free phosphorus or a binary compound of phosphorus, except with oxygen	C06B39/00	C06B39/00		129
C06B39/02	8	with an inorganic oxygen-halogen salt	C06B39/02	C06B39/02		9
C06B39/04	9	with a binary compound of phosphorus, except with oxygen	C06B39/04	C06B39/04		25
C06B39/06	8	with free metal, alloy, boron, silicon, selenium or tellurium	C06B39/06	C06B39/06		33
C06B41/00	7	Compositions containing a nitrated metallo-organic compound	C06B41/00	C06B41/00		98
C06B41/02	8	the compound containing lead	C06B41/02	C06B41/02		111
C06B41/04	9	with an organic explosive or an organic thermic component	C06B41/04	C06B41/04		14
C06B41/06	10	with an inorganic explosive or an inorganic thermic component	C06B41/06	C06B41/06		27
C06B41/08	9	with a metal azide or a metal fulminate	C06B41/08	C06B41/08		24
C06B41/10	9	with other nitrated metallo-organic compound	C06B41/10	C06B41/10		2
C06B43/00	7	Compositions characterised by explosive or thermic constituents not provided for in groups C06B25/00&#160;-&#160;C06B41/00	C06B43/00	C06B43/00		1456
C06B45/00	7	Compositions or products which are defined by structure or arrangement of component of product (explosive charges of particular form or shape F42B1/00, F42B3/00)	C06B45/00	C06B45/00		648
C06B45/02	8	comprising particles of diverse size or shape	C06B45/02	C06B45/02		159
C06B45/04	8	comprising solid particles dispersed in solid solution or matrix {not used for explosives where the matrix consists essentially of nitrated carbohydrates or a low molecular organic explosive}	C06B45/04	C06B45/04		71
C06B45/06	9	the solid solution or matrix containing an organic component	C06B45/06	C06B45/06		35
C06B45/08	10	the dispersed solid containing an inorganic explosive or an inorganic thermic component	C06B45/08	C06B45/08		33
C06B45/10	10	the organic component containing a resin	C06B45/10	C06B45/10		1552
C06B45/105	11	{The resin being a polymer bearing energetic groups or containing a soluble organic explosive}	C06B45/10	C06B45/10		642
C06B45/12	8	having contiguous layers or zones	C06B45/12	C06B45/12		454
C06B45/14	9	a layer or zone containing an inorganic explosive or an inorganic explosive or an inorganic thermic component	C06B45/14	C06B45/14		148
C06B45/16	10	the layer or zone containing at least one inorganic component from the group of azide, fulminate, phosphorus and phosphide	C06B45/16	C06B45/16		10
C06B45/18	8	comprising a coated component (particles dispersed in a matrix C06B45/04; coated explosive charges F42B)	C06B45/18	C06B45/18		143
C06B45/20	9	the component base containing an organic explosive or an organic thermic component	C06B45/20	C06B45/20		49
C06B45/22	10	the coating containing an organic compound	C06B45/22	C06B45/22		184
C06B45/24	11	the compound being an organic explosive or an organic thermic component	C06B45/24	C06B45/24		44
C06B45/26	12	the compound being a nitrated toluene	C06B45/26	C06B45/26		15
C06B45/28	10	the component base containing nitrocellulose and nitroglycerine	C06B45/28	C06B45/28		42
C06B45/30	9	the component base containing an inorganic explosive or an inorganic thermic component	C06B45/30	C06B45/30		135
C06B45/32	10	the coating containing an organic compound	C06B45/32	C06B45/32		250
C06B45/34	11	the compound being an organic explosive or an organic thermic component	C06B45/34	C06B45/34		89
C06B45/36	9	the component base containing both an organic explosive or thermic component and an inorganic explosive or thermic component	C06B45/36	C06B45/36		26
C06B47/00	7	Compositions in which the components are separately stored until the moment of burning or explosion, e.g. "Sprengel"-type explosives; Suspensions of solid component in a normally non-explosive liquid phase, including a thickened aqueous phase<br><br><u>NOTE</u><br><br>This group also covers emulsion type explosives in which a solid component is not compulsory	C06B47/00	C06B47/00		428
C06B47/02	8	the components comprising a binary propellant	C06B47/02	C06B47/02		134
C06B47/04	9	a component containing a nitrogen oxide or acid thereof	C06B47/04	C06B47/04		100
C06B47/06	9	a component being a liquefied normally gaseous material supplying oxygen (C06B47/04 takes precedence)	C06B47/06	C06B47/06		62
C06B47/08	9	a component containing hydrazine or a hydrazine derivative	C06B47/08	C06B47/08		196
C06B47/10	9	a component containing free boron, an organic borane or a binary compound of boron, except with oxygen	C06B47/10	C06B47/10		313
C06B47/12	9	a component being a liquefied normally gaseous fuel	C06B47/12	C06B47/12		57
C06B47/14	8	comprising a solid component and an aqueous phase	C06B47/14	C06B47/14		685
C06B47/145	9	{Water in oil emulsion type explosives in which a carbonaceous fuel forms the continuous phase}	C06B47/14	C06B47/14		495
C06B49/00	7	Use of single substances as explosives	C06B49/00	C06B49/00		105
